Note:
Before installing the executive program, proposed closing anti-virus software first strongly! 
Because in the course of installing, some antivirus software will delete or forbid the materials installed, 
make the installation fail or cut off.

Version Revision Record
===========================================
V1.2.0 (2026.06.09)
*. Supported Hardware model:
   -Writer: HY10000-WK08x (programming kit)
*. Supported Products:
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P51(HAO_2MHz), HY17P51(HAO_4MHz) , HY17P51(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
   -HY17P60B(HAO_5MHz), HY17P60B(HAO_10MHz)
   -HY17P68(HAO_5MHz), HY17P68(HAO_10MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Supported operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revision items:
   -Added configurable chip programming speed and read speed 
    settings. The default programming speed is 100KHz and the
    default read speed is 250 KHz if not specified. 
   -Added a configurable retry count for Verify failures. 
    The default retry count is 3 if not specified. 
   -Relocated the programming parameter storage area to prevent
    incorrect programming info. caused by Flash storage failures. 
   -Fixed bug: The WK08D programmer could still perform frequency
    calibration after the programming count limit had been reached.
   -Updated all of the include files. 
   -This version requires the WK08 programmer with Burner Transformer
    V1.9.0 or later (HY17P Series, firmware version: W17D03 or later).
===========================================
V1.1.9 (2024.10.23)
*. Supported Hardware model:
   -Writer: HY10000-WK08x (programming kit)
*. Supported Products:
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P51(HAO_2MHz), HY17P51(HAO_4MHz) , HY17P51(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
   -HY17P60(HAO_5MHz), HY17P60(HAO_10MHz)
   -HY17P68(HAO_5MHz), HY17P68(HAO_10MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Supported operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revision items:
   -Add-in Skip HAO Calibration Failure function. (Only support
    Writer firmware: WK08D W17D02.6 or later)
===========================================
V1.1.8 (2023.12.26)
*. Supported Hardware model:
   -Writer: HY10000-WK08x (programming kit)
*. Supported Products:
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P51(HAO_2MHz), HY17P51(HAO_4MHz) , HY17P51(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
   -HY17P60(HAO_5MHz), HY17P60(HAO_10MHz)
   -HY17P68(HAO_5MHz), HY17P68(HAO_10MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Supported operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revision items:
   -Fixed an abnormal problem caused by insufficient 
    permissions when downloading hex code.
===========================================
V1.1.7 (2023.10.26)
*. Supported Hardware model:
   -Writer: HY10000-WK08x (programming kit)
*. Supported Products:
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P51(HAO_2MHz), HY17P51(HAO_4MHz) , HY17P51(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
   -HY17P60(HAO_5MHz), HY17P60(HAO_10MHz)
   -HY17P68(HAO_5MHz), HY17P68(HAO_10MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Supported operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revision items:
   -Fixed an abnormal problem caused by insufficient permissions 
    when downloading hex code.
   -Updated the include files of HY17P52 series.
===========================================
V1.1.6 (2022.04.13)
*. Supported Hardware model:
   -Writer: HY10000-WK08x (programming kit)
*. Supported Products:
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P51(HAO_2MHz), HY17P51(HAO_4MHz) , HY17P51(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
   -HY17P60(HAO_5MHz), HY17P60(HAO_10MHz)
   -HY17P68(HAO_5MHz), HY17P68(HAO_10MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Supported operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revision items:
   -Updated the include files of HY17P58 series for HAO calibration.
===========================================
V1.1.5 (2021.09.08)
*. Supported Hardware model:
   -Writer: HY10000-WK08x (programming kit)
*. Supported Products:
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P51(HAO_2MHz), HY17P51(HAO_4MHz) , HY17P51(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
   -HY17P60(HAO_5MHz), HY17P60(HAO_10MHz)
   -HY17P68(HAO_5MHz), HY17P68(HAO_10MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Supported operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revision items:
   -Add-in "Writer ID function setting". 
   -Update All include's *. mem files.
   -Add HY17P6x series products.
   -Fix the HY17P4X/5X mem files to turn on TPS calibration function.
===========================================
V1.0 (2020.06.08)
*. Supported Hardware model:
   -Writer: HY10000-WK08C (programming kit)
   -Writer: HY10000-WK08D (programming kit)
*. Supported Products:
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Supported operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revision items:
   -Updated Include files
   -First Edition

