Note:
Before installing the executive program, proposed closing anti-virus software first strongly! 
Because in the course of installing, some antivirus software will delete or forbid the materials installed, 
make the installation fail or cut off.

Version Revision Record
===========================================
V1.1.2 (2023.07.03)
*. Supported Hardware model:
   -Writer: HY10000-WK09 (programming kit)
   -Firmware version:V1.0.12
*. Supported Products:
   -HY17P41(HAO_2MHz), HY17P41(HAO_4MHz) , HY17P41(HAO_8MHz)
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P51(HAO_2MHz), HY17P51(HAO_4MHz) , HY17P51(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
   -HY17P60(HAO_5MHz), HY17P60(HAO_10MHz)
   -HY17P60B(HAO_5MHz), HY17P60B(HAO_10MHz)
   -HY17P68(HAO_5MHz), HY17P68(HAO_10MHz)
   -HY17M24(HAO_2MHz), HY17M24(HAO_4MHz), HY17M24(HAO_8MHz), HY17M24(HAO_16MHz)
   -HY17M26(HAO_2MHz), HY17M26(HAO_4MHz), HY17M26(HAO_8MHz), HY17M26(HAO_16MHz)
   -HY17M28(HAO_2MHz), HY17M28(HAO_4MHz), HY17M28(HAO_8MHz), HY17M28(HAO_16MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -Optimize HAO calibration function.
   -Enhance the programming functions for HY17P41 & HY17M series.
   -Add the new functions of HAO SW Trim and LPO HW/SW trim for HY17M series.
   -Update Include files of HY17P41 & HY17M series.
===========================================
V1.1.0 (2022.10.07)
*. Supported Hardware model:
   -Writer: HY10000-WK09 (programming kit, writer)
   -Firmware version:V1.0.9
*. Supported Products:
   -HY17P41(HAO_2MHz), HY17P41(HAO_4MHz) , HY17P41(HAO_8MHz)
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P51(HAO_2MHz), HY17P51(HAO_4MHz) , HY17P51(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
   -HY17P60(HAO_5MHz), HY17P60(HAO_10MHz)
   -HY17P60B(HAO_5MHz), HY17P60B(HAO_10MHz)
   -HY17P68(HAO_5MHz), HY17P68(HAO_10MHz)
   -HY17M24(HAO_2MHz), HY17M24(HAO_4MHz), HY17M24(HAO_8MHz), HY17M24(HAO_16MHz)
   -HY17M26(HAO_2MHz), HY17M26(HAO_4MHz), HY17M26(HAO_8MHz), HY17M26(HAO_16MHz)
   -HY17M28(HAO_2MHz), HY17M28(HAO_4MHz), HY17M28(HAO_8MHz), HY17M28(HAO_16MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -Support Multi sites programming function.
   -Optimize Writer's Flash data storage mode to avoid abnormal data storage.
   -Optimize HAO calibration function.
   -Optimize the programming function to enhance the reliability of Writer.
   -Update Include files of HY17M24, HY17M26 & HY17M28 series.
===========================================
V1.05 (2022.04.13)
*. Supported Hardware model:
   -Writer: HY10000-WK09x
*. Supported Products:
   -HY17P41(HAO_2MHz), HY17P41(HAO_4MHz) , HY17P41(HAO_8MHz)
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P51(HAO_2MHz), HY17P51(HAO_4MHz) , HY17P51(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
   -HY17P60(HAO_5MHz), HY17P60(HAO_10MHz)
   -HY17P60B(HAO_5MHz), HY17P60B(HAO_10MHz)
   -HY17P68(HAO_5MHz), HY17P68(HAO_10MHz)
   -HY17M24(HAO_2MHz), HY17M24(HAO_4MHz), HY17M24(HAO_8MHz), HY17M24(HAO_16MHz)
   -HY17M26(HAO_2MHz), HY17M26(HAO_4MHz), HY17M26(HAO_8MHz), HY17M26(HAO_16MHz)
   -HY17M28(HAO_2MHz), HY17M28(HAO_4MHz), HY17M28(HAO_8MHz), HY17M28(HAO_16MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -Update Include files of HY17M24/HY17M26 & HY17P58 series.
   -Add HY17M28 series.
===========================================
V1.04 (2021.09.06)
*. Supported Hardware model:
   -Writer: HY10000-WK09x
*. Supported Products:
   -HY17P41(HAO_2MHz), HY17P41(HAO_4MHz) , HY17P41(HAO_8MHz)
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P51(HAO_2MHz), HY17P51(HAO_4MHz) , HY17P51(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
   -HY17P60(HAO_5MHz), HY17P60(HAO_10MHz)
   -HY17P60B(HAO_5MHz), HY17P60B(HAO_10MHz)
   -HY17P68(HAO_5MHz), HY17P68(HAO_10MHz)
   -HY17M24(HAO_2MHz), HY17M24(HAO_4MHz), HY17M24(HAO_8MHz), HY17M24(HAO_16MHz)
   -HY17M26(HAO_2MHz), HY17M26(HAO_4MHz), HY17M26(HAO_8MHz), HY17M26(HAO_16MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -Update Include files of HY17M26/HY17P68/HY17P51 series.
===========================================
V1.03 (2021.08.27)
*. Supported Hardware model:
   -Writer: HY10000-WK09x
*. Supported Products:
   -HY17P41(HAO_2MHz), HY17P41(HAO_4MHz) , HY17P41(HAO_8MHz)
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P51(HAO_2MHz), HY17P51(HAO_4MHz) , HY17P51(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
   -HY17P60(HAO_5MHz), HY17P60(HAO_10MHz)
   -HY17P60B(HAO_5MHz), HY17P60B(HAO_10MHz)
   -HY17P68(HAO_5MHz), HY17P68(HAO_10MHz)
   -HY17M24(HAO_2MHz), HY17M24(HAO_4MHz), HY17M24(HAO_8MHz), HY17M24(HAO_16MHz)
   -HY17M26(HAO_2MHz), HY17M26(HAO_4MHz), HY17M26(HAO_8MHz), HY17M26(HAO_16MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -Update Include files of HY17M24 & HY17M26 series.
   -Update HyUSB.dll to support all of Win OS.
===========================================
V1.02 (2021.08.18)
*. Supported Hardware model:
   -Writer: HY10000-WK09x
*. Supported Products:
   -HY17P41(HAO_2MHz), HY17P41(HAO_4MHz) , HY17P41(HAO_8MHz)
   -HY17P48(HAO_2MHz), HY17P48(HAO_4MHz) , HY17P48(HAO_8MHz)
   -HY17P51(HAO_2MHz), HY17P51(HAO_4MHz) , HY17P51(HAO_8MHz)
   -HY17P52(HAO_2MHz), HY17P52(HAO_4MHz) , HY17P52(HAO_8MHz)
   -HY17P55(HAO_2MHz), HY17P55(HAO_4MHz) , HY17P55(HAO_8MHz)
   -HY17P56(HAO_2MHz), HY17P56(HAO_4MHz) , HY17P56(HAO_8MHz)
   -HY17P58(HAO_2MHz), HY17P58(HAO_4MHz) , HY17P58(HAO_8MHz)
   -HY17P60(HAO_5MHz), HY17P60(HAO_10MHz)
   -HY17P60B(HAO_5MHz), HY17P60B(HAO_10MHz)
   -HY17P68(HAO_5MHz), HY17P68(HAO_10MHz)
   -HY17M24(HAO_2MHz), HY17M24(HAO_4MHz), HY17M24(HAO_8MHz), HY17M24(HAO_16MHz)
   -HY17M26(HAO_2MHz), HY17M26(HAO_4MHz), HY17M26(HAO_8MHz), HY17M26(HAO_16MHz)
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -First Edition