Note:
Before installing the executive program, proposed closing anti-virus software first strongly! 
Because in the course of installing, some antivirus software will delete or forbid the materials installed, 
make the installation fail or cut off.

Version Revision Record
===========================================
V1.9.0 (2026.06.22)
*. Supported Hardware model:
   -Writer: HY10000-WK08C & HY10000-WK08D
*. Supported Products:
   -HY10P Series, firmware version: W13AD1.8
   -HY11P Series, firmware version: WRIV2.50
   -HY12P Series, firmware version: WRIV2.50
   -HY13P Series, firmware version: W13AD1.6
   -HY15P Series, firmware version: W15P03.0
   -HY17P Series, firmware version: W17D03.1
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -HY17P Series: Relocated the original programming parameter 
    storage area to prevent incorrect programming information 
    caused by Flash storage failures.
   -Fixed bug: The WK08D programmer could still perform frequency 
    calibration even after the programming count limit had been
    exhausted.
   -Solve the problem of clearing the HAO calibration block size
    error when HAO calibration is not performed and skip HAO 
    Calibration Failure is selected.
   -Solve the problem of wrong setting of Chip code number.
   -Add new feature that when Skip HAO Calibration Failure is 
    selected, the program can be burned normally regardless of 
    whether HAO calibration is selected or not.
   -Add new feature that Customers can take the chip that failed 
    the HAO calibration before and select the Skip HAO calibrated
    function to continue burning the OTP code.
   -Fixed an issue that would cause programming errors when the 
    PC(Program Counter) function was not set.
   -Optimize the internal Flash storage function and extend the 
    storage life of Flash operations
   -Add new feature that allows users to choose whether to ignore 
    calibration failures and continue chip burning when HAO 
    calibration fails.
   -Fixed the HY17P6x series's SPI clock from 250khz to 100khz.
   -HY15P Series:
    1. Change the light signal to Busy after pressing the "Program" 
       button to avoid Checksum checking before burning.
    2. HAO calibration and code burning can be operated independently.
    3. When only doing HAO calibration, Delay1.5 seconds after the 
       calibration is completed before switching the light signal.
   -Fixed the issue of HY17P series FW burning error.
   -Optimize HY11P/HY12P series HAO calibration limits.
   -Enhance HY17P series Programming function as follows:
    1. Improve the programming method of Program Counter Function.
    2. Added the Writer's self-test function during programming, 
       that is, when the programming parameters are abnormal, 
       an error message (error22) will be prompted and the 
       programming will stop.
===========================================
V1.8.1 (2022.08.16)
*. Supported Hardware model:
   -Writer: HY10000-WK08C & HY10000-WK08D
*. Supported Products:
   -HY10P Series, firmware version: W13AD1.8
   -HY11P Series, firmware version: WRIV2.40
   -HY12P Series, firmware version: WRIV2.40
   -HY13P Series, firmware version: W13AD1.6
   -HY15P Series, firmware version: W15P02.6
   -HY17P Series, firmware version: W17D02.4
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -HY10P Series: Improve HAO calibration.
   -HY10P Series: Improve Verify Code function.
   -HY17P48: Improve HAO calibration.
   -Fixed the HY10P series's SPI R/W clock speed 
    from 500khz to 150khz.
===========================================
V1.7.9 (2022.05.16)
*. Supported Hardware model:
   -Writer: HY10000-WK08C & HY10000-WK08D
*. Supported Products:
   -HY10P Series, firmware version: W13AD1.6
   -HY11P Series, firmware version: WRIV2.40
   -HY12P Series, firmware version: WRIV2.40
   -HY13P Series, firmware version: W13AD1.6
   -HY15P Series, firmware version: W15P02.6
   -HY17P Series, firmware version: W17D02.3
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -Enhance HAO calibration function of HY17P.
===========================================
V1.7.8 (2021.07.30)
*. Supported Hardware model:
   -Writer: HY10000-WK08C & HY10000-WK08D
*. Supported Products:
   -HY10P Series, firmware version: W13AD1.6
   -HY11P Series, firmware version: WRIV2.40
   -HY12P Series, firmware version: WRIV2.40
   -HY13P Series, firmware version: W13AD1.6
   -HY15P Series, firmware version: W15P02.6
   -HY17P Series, firmware version: W17D02.2
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -Delete HY16F Series.
   -Fixed the HY17P series's SPI Write clock 
    from 140khz to 100khz.
   -Fixed the HY17P series's programming timing 
    for VDD connect 470uF capacitor applications.
   -Fix the HY17P SPI's programmed protocol from TYPE3 to TYPE2.
   -The SPI reading speed of HY17P series products is reduced from 
    4MHz to 250kHz to ensure the stability of data reading.
   -Enhance HY17P series Programming function
    (Add-in "Writer ID function setting").
   -Enhance HY15P series Programming function
    (Including TPS calibration and BIE block management).
   -Enhance HY16F series Programming function.
   -Speed up the HY15P series programming time.
   -Add Software's version control information.
   -Add HY17P6x series products.
   -Add TPS calibrated function for HY17P series.
===========================================
V1.60 (2020.06.08)
*. Supported Hardware model:
   -Writer: HY10000-WK08C (programming kit)
   -Writer: HY10000-WK08D (programming kit)
*. Supported Products:
   -HY10P Series, firmware version: W13AD1.6
   -HY11P Series, firmware version: WRIV2.40
   -HY12P Series, firmware version: WRIV2.40
   -HY13P Series, firmware version: W13AD1.6
   -HY15P Series, firmware version: W15P02.3
   -HY16F Series, firmware version: V4.2
   -HY17P Series, firmware version: W17D01.6
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -Fix HY17P48 HAO calibration function.
   -Fix HY17P series VDD programming voltage from 4.5V to 3.3V
   -Add rolling code function of  HY17P chip ID.
   -Speed up the HY17P series programming time.
   -Enhance HY16F series Programming function.
   -Fix the HY17P SPI's programmed protocol from TYPE3 to TYPE2.
   -Add Software's version control information.
===========================================
V1.50 (2018.11.13)
*. Supported Hardware model:
   -Writer: HY10000-WK08C & HY10000-WK08D
*. Supported Products:
   -HY10P Series, firmware version: W13AD1.6
   -HY11P Series, firmware version: WRIV2.40
   -HY12P Series, firmware version: WRIV2.40
   -HY13P Series, firmware version: W13AD1.6
   -HY15P Series, firmware version: W15P02.3
   -HY16F Series, firmware version: V3.4
   -HY17P Series, firmware version: W17D01.1
*. Minimum system requirements for software:
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -WinXP(32bit), Win7(32/64bit), Win8(32/64bit), Win10(32/64bit)
*. Communication interface
   -USB Port with HID-compliant device
*. Revised notes:
   -Add HY17P series product.
   -Fix the SPI clock as 125kHz for HY15P series.
   -Enhanced checksum verification method for HY15P53/43.
===========================================
V1.40 (2017.10.16)
*. Hardware support model: 
   -Writer: HY10000-WK08C
*. Support model:
   -HY10P Series, firmware version: W13AD1.6
   -HY11P Series, firmware version: WRIV2.40
   -HY12P Series, firmware version: WRIV2.40
   -HY13P Series, firmware version: W13AD1.6
   -HY15P Series, firmware version: W15P02.2
   -HY16F Series, firmware version: V3.4
*. Minimum system requirements for HYIDE program: 
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -Windows XP (32 bit)
   -Windows 7 (32/64 bit)
   -Windows 8 (32/64 bit)
   -Windows 10 (32/64 bit)
*. Communication interface
   -USB HID Port
*. Revision items:
   -Support HY15P41 product.
   -Added the rolling code function for HY11P/HY12P Series. 
   -Added the checksum backup to BIE for HY10P/HY13P Series.
   -Enhance the programming time of HY15P53 & HY15P43.

===========================================
V1.30 (2017.05.23)
*. Hardware support model: 
   -Writer: HY10000-WK08C
*. Support model:
   -HY10P Series, firmware version: W13AD1.5
   -HY11P Series, firmware version: WRIV2.30
   -HY12P Series, firmware version: WRIV2.30
   -HY13P Series, firmware version: W13AD1.5
   -HY15P Series, firmware version: W15P02.1
   -HY16F Series, firmware version: V3.4
*. Minimum system requirements for HYIDE program: 
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -Windows XP (32 bit)
   -Windows 7 (32/64 bit)
   -Windows 8 (32/64 bit)
   -Windows 10 (32/64 bit)
*. Communication interface
   -USB HID Port
*. Revision items:
   -Enhance function of "Encrypt & Decrypt" for HY16F Series.
   -Repair the security issues for HY16F Series.
   -Enhanced the WK08C's information 6 functions, can verify the SBM's
    checksum with the OTP,for HY10P/HY11P//HY12P/HY13P/HY15P series.
   -Added the WK08C's information 9 functions, can view the Data Bin's 
    szie & checksum,for HY16F series.
   -Added the WK08C's information 10 functions, can view the Data Bin's 
    write address begin,for HY16F series.
   -Fixed the HY11P/HY12P/HY13P series's programming timing 
    for VDD connect 470uF capacitor applications.
   -Documents update

===========================================
V1.20 (2016.11.11)
*. Hardware support model: 
   -Writer: HY10000-WK08C
*. Support model:
   -HY10P Series, firmware version: W13AD1.3
   -HY11P Series, firmware version: WRIV2.21
   -HY12P Series, firmware version: WRIV2.21
   -HY13P Series, firmware version: W13AD1.3
   -HY15P Series, firmware version: W15P02.0
   -HY16F Series, firmware version: V3.1
*. Minimum system requirements for HYIDE program: 
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -Windows XP(32 bit)
   -Windows 7 (32/64 bit)
   -Windows 8 (32/64 bit)
   -Windows 10 (32/64 bit)
*. Communication interface
   -USB HID Port
*. Revision items:
   -HY10P Series Addition Checksum Compare
   -HY11P/H12P Series Addition CheckSum Compare
   -HY13P Series Addition CheckSum Compare
   -HY15P Series Addition CheckSum Compare
                 VPP MAX. limit change to 9.30V
   -Documents update

===========================================
V1.10 (2016.08.17)
*. Hardware support model: 
   -Writer: HY10000-WK08C
*. Support model:
   -HY10P Series, firmware version: W13AD1.2
   -HY11P Series, firmware version: WRIV2.10
   -HY12P Series, firmware version: WRIV2.10
   -HY13P Series, firmware version: W13AD1.2
   -HY15P Series, firmware version: W15P01.9
   -HY16F Series, firmware version: V3.1
*. Minimum system requirements for HYIDE program: 
   -PC compatible PENTIUM system 
   -512MB memory size (recommended 1GB)
   -1 GB hard disc space
*. Support operation system: 
   -Windows XP(32 bit)
   -Windows 7 (32/64 bit)
   -Windows 8 (32/64 bit)
   -Windows 10 (32/64 bit)
*. Communication interface
   -USB HID Port
*. Revision items:
   -support checksum verify function at HY10P series.

===========================================
V1.00 (2016.07.28)
*. Hardware support model:
   -Writer: HY10000-WK08C
*. Support model:
   -HY10P Series,
   -HY11P Series,
   -HY12P Series,
   -HY13P Series,
   -HY15P Series,
   -HY16F Series,
*. Support operation system: 
   -Windows XP(32 bit)
   -Windows 7 (32/64 bit)
   -Windows 8 (32/64 bit)
   -Windows 10 (32/64 bit)
*. Communication interface
   -USB HID Port
